1. Clone the “Data\_Logger” repository to your GitHub Desktop

2. Install the CH340 Driver from <https://sparks.gogo.co.nz/ch340.html>

3. Install the Adafruit BNO055 library from the Library Manager

4. Wire the SPI SD card to the Arduino Nano using the pinout shown in the following website <https://learn.adafruit.com/adafruit-spi-flash-sd-card/arduino>

5.